(kicad_pcb (version 20170123) (host pcbnew "(2017-08-02 revision 9760937)-master")
  (general
    (thickness 1.6)
    (drawings 55)
    (tracks 722)
    (zones 0)
    (modules 64)
    (nets 130)
  )
  (page A4)
  (title_block
    (title "<Add project name here>")
    (date 2017-08-14)
  )
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.125)
    (pad_size 1.27 1.27)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 0 0)
    (grid_origin 126.9111 118.9863)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x0103c_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory plots))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 SYS_5V)
  (net 3 "Net-(Q2-Pad1)")
  (net 4 "Net-(Q2-Pad3)")
  (net 5 "Net-(Q1-Pad3)")
  (net 6 "Net-(Q1-Pad1)")
  (net 7 "Net-(Q3-Pad1)")
  (net 8 "Net-(Q3-Pad3)")
  (net 9 RESET#)
  (net 10 +3V3)
  (net 11 SPI_MOSI)
  (net 12 SPI_MISO)
  (net 13 SPI_CLK)
  (net 14 SPI_nCS)
  (net 15 "Net-(U3-Pad5)")
  (net 16 "Net-(X1-PadID)")
  (net 17 "Net-(C3-Pad1)")
  (net 18 PWM_BLUE)
  (net 19 PWM_GREEN)
  (net 20 PWM_RED)
  (net 21 "Net-(C4-Pad1)")
  (net 22 LDF1)
  (net 23 LDE1)
  (net 24 LDG1)
  (net 25 LDC2)
  (net 26 LDB2)
  (net 27 LDD2)
  (net 28 LDG2)
  (net 29 LDA2)
  (net 30 LDE2)
  (net 31 LDF2)
  (net 32 LDC1)
  (net 33 LDD1)
  (net 34 LDA1)
  (net 35 LDB1)
  (net 36 "Net-(RN1-Pad7)")
  (net 37 "Net-(RN1-Pad6)")
  (net 38 "Net-(RN1-Pad5)")
  (net 39 "Net-(RN2-Pad8)")
  (net 40 "Net-(RN2-Pad7)")
  (net 41 "Net-(RN2-Pad6)")
  (net 42 "Net-(RN2-Pad5)")
  (net 43 "Net-(U1-Pad14)")
  (net 44 "Net-(RN3-Pad8)")
  (net 45 "Net-(RN3-Pad7)")
  (net 46 "Net-(RN3-Pad6)")
  (net 47 "Net-(RN3-Pad5)")
  (net 48 "Net-(RN4-Pad8)")
  (net 49 "Net-(RN4-Pad7)")
  (net 50 "Net-(RN4-Pad6)")
  (net 51 "Net-(RN4-Pad5)")
  (net 52 "Net-(RN1-Pad8)")
  (net 53 "Net-(RN2-Pad4)")
  (net 54 "Net-(RN4-Pad4)")
  (net 55 "Net-(RN5-Pad1)")
  (net 56 "Net-(RN5-Pad8)")
  (net 57 ANALOG_IN)
  (net 58 ADC_GND)
  (net 59 ADC_PWR)
  (net 60 GPIO_BTN)
  (net 61 ACC_INT1)
  (net 62 UART0_RX)
  (net 63 UART0_TX)
  (net 64 I2C_SCL)
  (net 65 I2C_SDA)
  (net 66 USB1_D+)
  (net 67 USB1_D-)
  (net 68 USB1_VBUS)
  (net 69 ACC_INT2)
  (net 70 GNDPWR)
  (net 71 "Net-(FB4-Pad1)")
  (net 72 "Net-(R10-Pad1)")
  (net 73 "Net-(R9-Pad1)")
  (net 74 "Net-(R10-Pad2)")
  (net 75 "Net-(R9-Pad2)")
  (net 76 "Net-(LD1-Pad1)")
  (net 77 "Net-(LD1-Pad2)")
  (net 78 "Net-(LD1-Pad3)")
  (net 79 FTDI_3V3)
  (net 80 "Net-(U4-Pad4)")
  (net 81 "Net-(U4-Pad5)")
  (net 82 "Net-(U4-Pad11)")
  (net 83 "Net-(U4-Pad12)")
  (net 84 "Net-(U4-Pad14)")
  (net 85 "Net-(U4-Pad16)")
  (net 86 "Net-(U3-Pad3)")
  (net 87 PWR#)
  (net 88 "Net-(P1-Pad12)")
  (net 89 "Net-(P1-Pad10)")
  (net 90 "Net-(P1-Pad8)")
  (net 91 "Net-(P1-Pad6)")
  (net 92 "Net-(P2-Pad3)")
  (net 93 "Net-(P1-Pad4)")
  (net 94 "Net-(P1-Pad2)")
  (net 95 DBG_VBUS)
  (net 96 "Net-(P2-Pad36)")
  (net 97 "Net-(P2-Pad35)")
  (net 98 "Net-(P2-Pad34)")
  (net 99 "Net-(P2-Pad32)")
  (net 100 "Net-(P2-Pad30)")
  (net 101 "Net-(P2-Pad28)")
  (net 102 "Net-(P2-Pad24)")
  (net 103 "Net-(P2-Pad22)")
  (net 104 "Net-(P2-Pad20)")
  (net 105 "Net-(P2-Pad19)")
  (net 106 "Net-(P2-Pad18)")
  (net 107 "Net-(P2-Pad17)")
  (net 108 "Net-(P2-Pad16)")
  (net 109 "Net-(P2-Pad14)")
  (net 110 "Net-(P2-Pad13)")
  (net 111 "Net-(P2-Pad11)")
  (net 112 "Net-(P2-Pad10)")
  (net 113 "Net-(P2-Pad9)")
  (net 114 "Net-(P2-Pad8)")
  (net 115 "Net-(P2-Pad7)")
  (net 116 "Net-(P2-Pad6)")
  (net 117 "Net-(P2-Pad5)")
  (net 118 "Net-(P2-Pad4)")
  (net 119 "Net-(P2-Pad2)")
  (net 120 "Net-(P1-Pad29)")
  (net 121 "Net-(P1-Pad27)")
  (net 122 "Net-(P1-Pad25)")
  (net 123 "Net-(P1-Pad23)")
  (net 124 "Net-(P1-Pad21)")
  (net 125 "Net-(P1-Pad20)")
  (net 126 PWM_RED_ALT)
  (net 127 "Net-(U5-Pad3)")
  (net 128 USB1_DRV_VBUS)
  (net 129 "Net-(P1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net ACC_INT1)
    (add_net ACC_INT2)
    (add_net ADC_GND)
    (add_net ADC_PWR)
    (add_net ANALOG_IN)
    (add_net DBG_VBUS)
    (add_net FTDI_3V3)
    (add_net GND)
    (add_net GNDPWR)
    (add_net GPIO_BTN)
    (add_net I2C_SCL)
    (add_net I2C_SDA)
    (add_net LDA1)
    (add_net LDA2)
    (add_net LDB1)
    (add_net LDB2)
    (add_net LDC1)
    (add_net LDC2)
    (add_net LDD1)
    (add_net LDD2)
    (add_net LDE1)
    (add_net LDE2)
    (add_net LDF1)
    (add_net LDF2)
    (add_net LDG1)
    (add_net LDG2)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(FB4-Pad1)")
    (add_net "Net-(LD1-Pad1)")
    (add_net "Net-(LD1-Pad2)")
    (add_net "Net-(LD1-Pad3)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad20)")
    (add_net "Net-(P1-Pad21)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad25)")
    (add_net "Net-(P1-Pad27)")
    (add_net "Net-(P1-Pad29)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad11)")
    (add_net "Net-(P2-Pad13)")
    (add_net "Net-(P2-Pad14)")
    (add_net "Net-(P2-Pad16)")
    (add_net "Net-(P2-Pad17)")
    (add_net "Net-(P2-Pad18)")
    (add_net "Net-(P2-Pad19)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad20)")
    (add_net "Net-(P2-Pad22)")
    (add_net "Net-(P2-Pad24)")
    (add_net "Net-(P2-Pad28)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad30)")
    (add_net "Net-(P2-Pad32)")
    (add_net "Net-(P2-Pad34)")
    (add_net "Net-(P2-Pad35)")
    (add_net "Net-(P2-Pad36)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P2-Pad9)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(RN1-Pad5)")
    (add_net "Net-(RN1-Pad6)")
    (add_net "Net-(RN1-Pad7)")
    (add_net "Net-(RN1-Pad8)")
    (add_net "Net-(RN2-Pad4)")
    (add_net "Net-(RN2-Pad5)")
    (add_net "Net-(RN2-Pad6)")
    (add_net "Net-(RN2-Pad7)")
    (add_net "Net-(RN2-Pad8)")
    (add_net "Net-(RN3-Pad5)")
    (add_net "Net-(RN3-Pad6)")
    (add_net "Net-(RN3-Pad7)")
    (add_net "Net-(RN3-Pad8)")
    (add_net "Net-(RN4-Pad4)")
    (add_net "Net-(RN4-Pad5)")
    (add_net "Net-(RN4-Pad6)")
    (add_net "Net-(RN4-Pad7)")
    (add_net "Net-(RN4-Pad8)")
    (add_net "Net-(RN5-Pad1)")
    (add_net "Net-(RN5-Pad8)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(X1-PadID)")
    (add_net PWM_BLUE)
    (add_net PWM_GREEN)
    (add_net PWM_RED)
    (add_net PWM_RED_ALT)
    (add_net PWR#)
    (add_net RESET#)
    (add_net SPI_CLK)
    (add_net SPI_MISO)
    (add_net SPI_MOSI)
    (add_net SPI_nCS)
    (add_net SYS_5V)
    (add_net UART0_RX)
    (add_net UART0_TX)
    (add_net USB1_D+)
    (add_net USB1_D-)
    (add_net USB1_DRV_VBUS)
    (add_net USB1_VBUS)
  )
  (module PocketBeagle.pretty:FIDUCIAL_40MIL (layer Top) (tedit 59925435)
    (at 173.5201 93.6117)
    (attr smd)
    (fp_text reference *G2 (at 0.3 2.1) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL (at -0.1 -2.2) (layer F.SilkS) hide)
    (pad P$1 smd circle (at 0 0) (size 1.016 1.016) (layers Top F.Mask)
      (solder_mask_margin 0.35) (clearance 0.35))
  )
  (module PocketBeagle.pretty:FIDUCIAL_40MIL (layer Top) (tedit 59925435)
    (at 123.7107 116.5987)
    (attr smd)
    (fp_text reference *G1 (at 0.3 2.1) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL (at -0.1 -2.2) (layer F.SilkS) hide)
    (pad P$1 smd circle (at 0 0) (size 1.016 1.016) (layers Top F.Mask)
      (solder_mask_margin 0.35) (clearance 0.35))
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 5A8485FB)
    (at 148.3741 113.9571)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 2.2098 0.9906) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 2 SYS_5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A8485F3)
    (at 144.6403 113.8047 270)
    (attr smd)
    (fp_text reference R13 (at 0.0254 -1.0668 270) (layer F.SilkS))
    (fp_text value 4.7K (at 3.048 -1.00584 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0 270) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 128 USB1_DRV_VBUS))
    (pad 2 smd rect (at 0.49784 0 270) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer Top) (tedit 5A828339)
    (at 142.1257 112.3569)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at -0.254 -2.1336) (layer F.SilkS))
    (fp_text value TPS2051C (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 68 USB1_VBUS))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 127 "Net-(U5-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 128 USB1_DRV_VBUS))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 2 SYS_5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PocketBeagle.pretty:LED_RGB_PLLC-6 (layer Top) (tedit 5A81A95F)
    (at 155.4861 104.7877 90)
    (descr "RGB LED PLLC-6")
    (tags "RGB LED PLLC-6")
    (attr smd)
    (fp_text reference LD1 (at -0.762 -3.1496 90) (layer F.SilkS))
    (fp_text value LED_BGR (at 0.03 3.37 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 -1.8 180) (size 1.4 2) (layers Top F.Paste F.Mask)
      (net 76 "Net-(LD1-Pad1)"))
    (pad 2 smd rect (at -2.2 0 180) (size 1 2) (layers Top F.Paste F.Mask)
      (net 77 "Net-(LD1-Pad2)"))
    (pad 3 smd rect (at -2.2 1.8 180) (size 1.4 2) (layers Top F.Paste F.Mask)
      (net 78 "Net-(LD1-Pad3)"))
    (pad 4 smd rect (at 2.2 1.8 180) (size 1.4 2) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 5 smd rect (at 2.2 0 180) (size 1 2) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 6 smd rect (at 2.2 -1.8 180) (size 1.4 2) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module "PocketBeagle.pretty:TH-2X18-(35MIL-DIA)-W_O-SILK" (layer Top) (tedit 59924F19)
    (at 148.5011 117.7036)
    (attr virtual)
    (fp_text reference P1 (at -18.68678 3.34518) (layer F.SilkS))
    (fp_text value ~ (at 0 0) (layer F.SilkS))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 PWM_BLUE))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 126 PWM_RED_ALT))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 61 ACC_INT1))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 PWM_GREEN))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 62 UART0_RX))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 69 ACC_INT2))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 63 UART0_TX))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(P1-Pad29)"))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 64 I2C_SCL))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(P1-Pad27)"))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 65 I2C_SDA))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(P1-Pad25)"))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 SYS_5V))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(P1-Pad23)"))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(P1-Pad21)"))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(P1-Pad20)"))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 57 ANALOG_IN))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 ADC_PWR))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 58 ADC_GND))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3V3))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(P1-Pad12)"))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 66 USB1_D+))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(P1-Pad10)"))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 67 USB1_D-))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(P1-Pad8)"))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(P1-Pad7)"))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(P1-Pad6)"))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 68 USB1_VBUS))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(P1-Pad4)"))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 128 USB1_DRV_VBUS))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 95 DBG_VBUS))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A75475E)
    (at 134.80542 99.82708 90)
    (attr smd)
    (fp_text reference R12 (at -0.04318 -0.83058 90) (layer F.SilkS))
    (fp_text value 4.7K (at 3.048 -1.00584 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0 90) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 126 PWM_RED_ALT))
    (pad 2 smd rect (at 0.49784 0 90) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 7 "Net-(Q3-Pad1)"))
  )
  (module PocketBeagle.pretty:MINI_PUSHBUTTON (layer Top) (tedit 5A74BB12)
    (at 159.09036 98.49866 90)
    (attr smd)
    (fp_text reference SW2 (at 0.07112 -1.95072 90) (layer F.SilkS))
    (fp_text value BTN (at 0.80772 2.36474 90) (layer F.SilkS) hide)
    (pad 4 smd rect (at 1.99898 0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.99898 0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.99898 -0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 87 PWR#))
    (pad 1 smd rect (at -1.99898 -0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 87 PWR#))
  )
  (module PocketBeagle.pretty:MINI_PUSHBUTTON (layer Top) (tedit 5A74BB16)
    (at 163.53536 98.49866 90)
    (attr smd)
    (fp_text reference SW3 (at 0.0254 -1.96596 90) (layer F.SilkS))
    (fp_text value BTN (at 0.80772 2.36474 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.99898 -0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 9 RESET#))
    (pad 2 smd rect (at 1.99898 -0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 9 RESET#))
    (pad 3 smd rect (at -1.99898 0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.99898 0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module PocketBeagle.pretty:MMA8452QR1 (layer Top) (tedit 5A7401D7)
    (at 161.05378 103.84536 90)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U2 (at -1.67894 -2.26568 180) (layer F.SilkS))
    (fp_text value MMA8452QR1 (at 0 2.85 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.275 -1 90) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 2 smd rect (at -1.275 -0.5 90) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -1.275 0 90) (size 0.813 0.305) (layers Top F.Paste F.Mask))
    (pad 4 smd rect (at -1.275 0.5 90) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 64 I2C_SCL))
    (pad 5 smd rect (at -1.275 1 90) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -0.5 1.275 180) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 65 I2C_SDA))
    (pad 7 smd rect (at 0 1.275 180) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.5 1.275 180) (size 0.813 0.305) (layers Top F.Paste F.Mask))
    (pad 9 smd rect (at 1.275 1 90) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 69 ACC_INT2))
    (pad 10 smd rect (at 1.275 0.5 90) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 1.275 0 90) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 61 ACC_INT1))
    (pad 12 smd rect (at 1.275 -0.5 90) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 1.275 -1 90) (size 0.813 0.305) (layers Top F.Paste F.Mask))
    (pad 14 smd rect (at 0.5 -1.275 180) (size 0.813 0.305) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 15 smd rect (at 0 -1.275 180) (size 0.813 0.305) (layers Top F.Paste F.Mask))
    (pad 16 smd rect (at -0.5 -1.275 180) (size 0.813 0.305) (layers Top F.Paste F.Mask))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PocketBeagle.pretty:3352T-1 (layer Top) (tedit 5A73F38C)
    (at 169.291 99.695 270)
    (fp_text reference RV1 (at -4.40436 1.30048) (layer F.SilkS))
    (fp_text value 3352T-1-502LF (at 0 4.699 270) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 58 ADC_GND))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 57 ANALOG_IN))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 59 ADC_PWR))
    (model /home/michael/3352T-1.wrl
      (at (xyz 0 0.115 0.025))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_A (layer Top) (tedit 5A7540D1)
    (at 132.26288 101.95814 270)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J1 (at -6.28 10.16 270) (layer F.SilkS))
    (fp_text value USB_A (at 3.83794 7.43458 270) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 7.11286 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 4.57286 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 66 USB1_D+))
    (pad 2 thru_hole circle (at 2.54086 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 67 USB1_D-))
    (pad 1 thru_hole circle (at 0.00086 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(FB4-Pad1)"))
    (pad 5 thru_hole circle (at 10.16086 2.66488 180) (size 2.99974 2.99974) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 70 GNDPWR))
    (pad 5 thru_hole circle (at -3.55514 2.66488 180) (size 2.99974 2.99974) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 70 GNDPWR))
    (model Connect.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 5A71F804)
    (at 161.5186 106.8324)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at -0.0508 0.9906) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 5A71F807)
    (at 169.36 112.014 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0.069 -1.143 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.7 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 21 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 5A71F845)
    (at 160.909 109.305 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0.04318 1.0398 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 79 FTDI_3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 5A71F850)
    (at 164.084 114.046 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at -0.01656 -1.04376 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 79 FTDI_3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 5A848162)
    (at 139.3825 111.5949 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 1.7526 -0.0254 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 68 USB1_VBUS))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 5A71F84D)
    (at 160.909 112.6998 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at -1.64846 -0.01016 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 95 DBG_VBUS))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 5A71F840)
    (at 159.5501 107.1753 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at -0.1016 0.889 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_4x4mm_Pitch0.65mm (layer Top) (tedit 5A71F2EC)
    (at 164.602 110.49 180)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.65")
    (attr smd)
    (fp_text reference U4 (at -2.89542 -1.96902 180) (layer F.SilkS))
    (fp_text value FT230XQ (at 0 3.4 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 -0.975 180) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 79 FTDI_3V3))
    (pad 2 smd rect (at -2 -0.325 180) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 63 UART0_TX))
    (pad 3 smd rect (at -2 0.325 180) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2 0.975 180) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 80 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -0.975 2 270) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 81 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at -0.325 2 270) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 74 "Net-(R10-Pad2)"))
    (pad 7 smd rect (at 0.325 2 270) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 75 "Net-(R9-Pad2)"))
    (pad 8 smd rect (at 0.975 2 270) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 79 FTDI_3V3))
    (pad 9 smd rect (at 2 0.975 180) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 79 FTDI_3V3))
    (pad 10 smd rect (at 2 0.325 180) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 95 DBG_VBUS))
    (pad 11 smd rect (at 2 -0.325 180) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 82 "Net-(U4-Pad11)"))
    (pad 12 smd rect (at 2 -0.975 180) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 83 "Net-(U4-Pad12)"))
    (pad 13 smd rect (at 0.975 -2 270) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 0.325 -2 270) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 84 "Net-(U4-Pad14)"))
    (pad 15 smd rect (at -0.325 -2 270) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 62 UART0_RX))
    (pad 16 smd rect (at -0.975 -2 270) (size 0.8 0.35) (layers Top F.Paste F.Mask)
      (net 85 "Net-(U4-Pad16)"))
    (pad 17 smd rect (at 0.625 0.625 180) (size 1.25 1.25) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.625 -0.625 180) (size 1.25 1.25) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.625 0.625 180) (size 1.25 1.25) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.625 -0.625 180) (size 1.25 1.25) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A82750D)
    (at 149.606 98.552 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD15 (at -0.2 1.3589 180) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 25 LDC2))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F836)
    (at 152.09266 96.15424)
    (attr smd)
    (fp_text reference R11 (at -0.0889 -0.85852) (layer F.SilkS))
    (fp_text value 4.7K (at 3.048 -1.00584) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 60 GPIO_BTN))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F9F9)
    (at 169.78672 110.871 180)
    (attr smd)
    (fp_text reference R9 (at 1.51172 0.09208 180) (layer F.SilkS))
    (fp_text value 22 (at 0.43 -2.51 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 73 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 75 "Net-(R9-Pad2)"))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F839)
    (at 164.6936 104.3178 180)
    (attr smd)
    (fp_text reference R8 (at -1.51416 -0.01 180) (layer F.SilkS))
    (fp_text value 4.7K (at 3.048 -1.00584 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 65 I2C_SDA))
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F9FE)
    (at 169.79392 109.93374 180)
    (attr smd)
    (fp_text reference R10 (at 1.64592 -0.04826 180) (layer F.SilkS))
    (fp_text value 22 (at 0.55 3.23 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 72 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 74 "Net-(R10-Pad2)"))
  )
  (module PocketBeagle.pretty:0603 (layer Top) (tedit 200000)
    (at 169.291 114.173 180)
    (attr smd)
    (fp_text reference FB3 (at 2.3331 -0.05678 180) (layer F.SilkS))
    (fp_text value ~ (at 3.048 -1.2065 180) (layer F.SilkS))
    (pad 2 smd rect (at 0.84836 0 180) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 95 DBG_VBUS))
    (pad 1 smd rect (at -0.84836 0 180) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 21 "Net-(C4-Pad1)"))
  )
  (module PocketBeagle.pretty:0603 (layer Top) (tedit 200000)
    (at 134.81558 111.4933 90)
    (attr smd)
    (fp_text reference FB2 (at 2.3622 -0.00508 90) (layer F.SilkS))
    (fp_text value ~ (at 3.048 -1.2065 90) (layer F.SilkS))
    (pad 2 smd rect (at 0.84836 0 90) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.84836 0 90) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 70 GNDPWR))
  )
  (module PocketBeagle.pretty:0603 (layer Top) (tedit 200000)
    (at 134.7851 102.86492 270)
    (attr smd)
    (fp_text reference FB4 (at 2.43078 0.0254 270) (layer F.SilkS))
    (fp_text value ~ (at 3.048 -1.2065 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.84836 0 270) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 71 "Net-(FB4-Pad1)"))
    (pad 2 smd rect (at 0.84836 0 270) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 68 USB1_VBUS))
  )
  (module RN0804 (layer Top) (tedit 5A71F3A8)
    (at 155.1051 109.0803)
    (attr smd)
    (fp_text reference RN5 (at 2.063 -0.02) (layer F.SilkS))
    (fp_text value 470 (at 0.147857 1.96417) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8001 0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 55 "Net-(RN5-Pad1)"))
    (pad 2 smd rect (at -0.24892 0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad3)"))
    (pad 3 smd rect (at 0.24892 0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 4 "Net-(Q2-Pad3)"))
    (pad 4 smd rect (at 0.8001 0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 8 "Net-(Q3-Pad3)"))
    (pad 5 smd rect (at 0.8001 -0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 78 "Net-(LD1-Pad3)"))
    (pad 6 smd rect (at 0.24892 -0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 77 "Net-(LD1-Pad2)"))
    (pad 7 smd rect (at -0.24892 -0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 76 "Net-(LD1-Pad1)"))
    (pad 8 smd rect (at -0.8001 -0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 56 "Net-(RN5-Pad8)"))
  )
  (module RN0804 (layer Top) (tedit 5A71F429)
    (at 143.56 105.07 90)
    (attr smd)
    (fp_text reference RN4 (at 0.0029 1.3597 270) (layer F.SilkS))
    (fp_text value 470 (at -0.002143 1.88417 90) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 48 "Net-(RN4-Pad8)"))
    (pad 7 smd rect (at -0.24892 -0.49784 90) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 49 "Net-(RN4-Pad7)"))
    (pad 6 smd rect (at 0.24892 -0.49784 90) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 50 "Net-(RN4-Pad6)"))
    (pad 5 smd rect (at 0.8001 -0.49784 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 51 "Net-(RN4-Pad5)"))
    (pad 4 smd rect (at 0.8001 0.49784 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 54 "Net-(RN4-Pad4)"))
    (pad 3 smd rect (at 0.24892 0.49784 90) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 24 LDG1))
    (pad 2 smd rect (at -0.24892 0.49784 90) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 22 LDF1))
    (pad 1 smd rect (at -0.8001 0.49784 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 23 LDE1))
  )
  (module RN0804 (layer Top) (tedit 5A71F3AD)
    (at 140.46 108.23)
    (attr smd)
    (fp_text reference RN3 (at -0.01 1.371) (layer F.SilkS))
    (fp_text value 470 (at 0.277857 1.98417) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8001 0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 34 LDA1))
    (pad 2 smd rect (at -0.24892 0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 35 LDB1))
    (pad 3 smd rect (at 0.24892 0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 32 LDC1))
    (pad 4 smd rect (at 0.8001 0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 33 LDD1))
    (pad 5 smd rect (at 0.8001 -0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 47 "Net-(RN3-Pad5)"))
    (pad 6 smd rect (at 0.24892 -0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 46 "Net-(RN3-Pad6)"))
    (pad 7 smd rect (at -0.24892 -0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 45 "Net-(RN3-Pad7)"))
    (pad 8 smd rect (at -0.8001 -0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 44 "Net-(RN3-Pad8)"))
  )
  (module RN0804 (layer Top) (tedit 5A71F3FF)
    (at 138.73 100.84 180)
    (attr smd)
    (fp_text reference RN2 (at -0.208 1.272 180) (layer F.SilkS))
    (fp_text value 470 (at -0.002143 1.82417 180) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 39 "Net-(RN2-Pad8)"))
    (pad 7 smd rect (at -0.24892 -0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 40 "Net-(RN2-Pad7)"))
    (pad 6 smd rect (at 0.24892 -0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 41 "Net-(RN2-Pad6)"))
    (pad 5 smd rect (at 0.8001 -0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 42 "Net-(RN2-Pad5)"))
    (pad 4 smd rect (at 0.8001 0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 53 "Net-(RN2-Pad4)"))
    (pad 3 smd rect (at 0.24892 0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 28 LDG2))
    (pad 2 smd rect (at -0.24892 0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 31 LDF2))
    (pad 1 smd rect (at -0.8001 0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 30 LDE2))
  )
  (module RN0804 (layer Top) (tedit 5A71F3B4)
    (at 141.14 100.84 180)
    (attr smd)
    (fp_text reference RN1 (at -0.084 1.272 180) (layer F.SilkS))
    (fp_text value 470 (at -0.032143 1.92417 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8001 0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 29 LDA2))
    (pad 2 smd rect (at -0.24892 0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 26 LDB2))
    (pad 3 smd rect (at 0.24892 0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 25 LDC2))
    (pad 4 smd rect (at 0.8001 0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 27 LDD2))
    (pad 5 smd rect (at 0.8001 -0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 38 "Net-(RN1-Pad5)"))
    (pad 6 smd rect (at 0.24892 -0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 37 "Net-(RN1-Pad6)"))
    (pad 7 smd rect (at -0.24892 -0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 36 "Net-(RN1-Pad7)"))
    (pad 8 smd rect (at -0.8001 -0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 52 "Net-(RN1-Pad8)"))
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 5A71F831)
    (at 136.50214 101.80828 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 1.778 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer Top) (tedit 5A71F2F2)
    (at 139.94 104.59 270)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at -2.228 -3.316) (layer F.SilkS))
    (fp_text value MCP23S18-E/MJ (at 0 3.375 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.95 -1.25 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 36 "Net-(RN1-Pad7)"))
    (pad 2 smd rect (at -1.95 -0.75 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 37 "Net-(RN1-Pad6)"))
    (pad 3 smd rect (at -1.95 -0.25 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 38 "Net-(RN1-Pad5)"))
    (pad 4 smd rect (at -1.95 0.25 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 39 "Net-(RN2-Pad8)"))
    (pad 5 smd rect (at -1.95 0.75 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 40 "Net-(RN2-Pad7)"))
    (pad 6 smd rect (at -1.95 1.25 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 41 "Net-(RN2-Pad6)"))
    (pad 7 smd rect (at -1.25 1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 42 "Net-(RN2-Pad5)"))
    (pad 8 smd rect (at -0.75 1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 9 smd rect (at -0.25 1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 14 SPI_nCS))
    (pad 10 smd rect (at 0.25 1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 13 SPI_CLK))
    (pad 11 smd rect (at 0.75 1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 11 SPI_MOSI))
    (pad 12 smd rect (at 1.25 1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 12 SPI_MISO))
    (pad 13 smd rect (at 1.95 1.25 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 9 RESET#))
    (pad 14 smd rect (at 1.95 0.75 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 43 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.95 0.25 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 44 "Net-(RN3-Pad8)"))
    (pad 16 smd rect (at 1.95 -0.25 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 45 "Net-(RN3-Pad7)"))
    (pad 17 smd rect (at 1.95 -0.75 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 46 "Net-(RN3-Pad6)"))
    (pad 18 smd rect (at 1.95 -1.25 270) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 47 "Net-(RN3-Pad5)"))
    (pad 19 smd rect (at 1.25 -1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 48 "Net-(RN4-Pad8)"))
    (pad 20 smd rect (at 0.75 -1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 49 "Net-(RN4-Pad7)"))
    (pad 21 smd rect (at 0.25 -1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 50 "Net-(RN4-Pad6)"))
    (pad 22 smd rect (at -0.25 -1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 51 "Net-(RN4-Pad5)"))
    (pad 23 smd rect (at -0.75 -1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -1.25 -1.95) (size 0.85 0.3) (layers Top F.Paste F.Mask)
      (net 52 "Net-(RN1-Pad8)"))
    (pad 25 smd rect (at 0.65 0.65 270) (size 1.3 1.3) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65 270) (size 1.3 1.3) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65 270) (size 1.3 1.3) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65 270) (size 1.3 1.3) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A82753B)
    (at 150.876 109.32 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD6 (at 0 -1.38 270) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 33 LDD1))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827553)
    (at 149.606 111.506 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD3 (at -0.0381 -1.3589 180) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 23 LDE1))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827540)
    (at 148.082 109.31 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD5 (at 0 -1.322 270) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 24 LDG1))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A8273C3)
    (at 146.5453 107.13 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD7 (at -0.254 1.3517 180) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 35 LDB1))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827537)
    (at 149.5933 107.15 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD8 (at 0.0254 1.3971 180) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 32 LDC1))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827528)
    (at 146.558 102.87 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD9 (at -0.0381 -1.3843 180) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 31 LDF2))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A82752F)
    (at 149.606 102.87 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD10 (at 0.0127 -1.3843 180) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 30 LDE2))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827523)
    (at 145.288 100.711 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD11 (at 0 -1.27 270) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 29 LDA2))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827519)
    (at 148.082 100.72 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD12 (at 0 -1.352 270) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 28 LDG2))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827513)
    (at 150.876 100.69 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD13 (at 0 -1.27 270) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 27 LDD2))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A82750A)
    (at 146.558 98.552 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD14 (at -0.1397 1.3335 180) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 26 LDB2))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827548)
    (at 145.288 109.3216 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD4 (at -0.0127 -1.3081 270) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 34 LDA1))
  )
  (module LEDs:LED-0603 (layer Top) (tedit 5A827550)
    (at 146.558 111.506 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD2 (at -0.0127 -1.3335 180) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 22 LDF1))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F869)
    (at 164.6936 105.6386 180)
    (attr smd)
    (fp_text reference R7 (at -1.532 -0.01 180) (layer F.SilkS))
    (fp_text value 4.7K (at 3.048 -1.00584 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 10 +3V3))
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 64 I2C_SCL))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F85D)
    (at 134.80796 97.91446 270)
    (attr smd)
    (fp_text reference R6 (at 0 0.762 270) (layer F.SilkS))
    (fp_text value 100K (at 3.048 -1.00584 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 270) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.49784 0 270) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 7 "Net-(Q3-Pad1)"))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F529)
    (at 152.44248 113.94948 180)
    (attr smd)
    (fp_text reference R4 (at 0.0628 -0.96774 180) (layer F.SilkS))
    (fp_text value 100K (at 3.048 -1.00584 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F83D)
    (at 134.80796 96.00946 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.762 270) (layer F.SilkS))
    (fp_text value 4.7K (at 3.048 -1.00584 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 270) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 7 "Net-(Q3-Pad1)"))
    (pad 1 smd rect (at -0.49784 0 270) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 20 PWM_RED))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F866)
    (at 158.78302 113.92916 180)
    (attr smd)
    (fp_text reference R2 (at 0.02794 -0.94234 180) (layer F.SilkS))
    (fp_text value 4.7K (at 3.048 -1.00584 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 19 PWM_GREEN))
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 3 "Net-(Q2-Pad1)"))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F4EE)
    (at 154.38248 113.92948 180)
    (attr smd)
    (fp_text reference R1 (at -0.14096 -0.9217 180) (layer F.SilkS))
    (fp_text value 4.7K (at 3.048 -1.00584 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad1)"))
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 18 PWM_BLUE))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 5A71F863)
    (at 156.86818 113.92916 180)
    (attr smd)
    (fp_text reference R5 (at -0.0962 -0.95758 180) (layer F.SilkS))
    (fp_text value 100K (at 3.048 -1.00584 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 3 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module PocketBeagle.pretty:0603 (layer Top) (tedit 200000)
    (at 169.32656 106.62158 180)
    (attr smd)
    (fp_text reference FB1 (at 2.258 0.03 180) (layer F.SilkS))
    (fp_text value ~ (at 3.048 -1.2065 180) (layer F.SilkS))
    (pad 2 smd rect (at 0.84836 0 180) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.84836 0 180) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 70 GNDPWR))
  )
  (module "PocketBeagle.pretty:10118192-0001LF(MICRO-USB-B-AMPHENOL-FCI)" (layer Top) (tedit 5A71F2E5)
    (at 174.54 110.32888 90)
    (attr smd)
    (fp_text reference X1 (at -5.43112 -0.37) (layer F.SilkS))
    (fp_text value 10118192-0001LF (at 0.81 9.47) (layer F.SilkS) hide)
    (fp_text user "Edge of PCB" (at 1.397 1.47066 90) (layer F.SilkS))
    (pad CGND smd rect (at -3.79984 0 90) (size 1.79832 1.89992) (layers Top F.Paste F.Mask)
      (net 70 GNDPWR))
    (pad CGND smd rect (at -1.19888 0 90) (size 1.89992 1.89992) (layers Top F.Paste F.Mask)
      (net 70 GNDPWR))
    (pad CGND smd rect (at 1.19888 0 90) (size 1.89992 1.89992) (layers Top F.Paste F.Mask)
      (net 70 GNDPWR))
    (pad CGND smd rect (at 3.79984 0 90) (size 1.79832 1.89992) (layers Top F.Paste F.Mask)
      (net 70 GNDPWR))
    (pad CGND smd rect (at 3.0988 -2.54762 90) (size 2.09804 1.59766) (layers Top F.Paste F.Mask)
      (net 70 GNDPWR))
    (pad CGND smd rect (at -3.0988 -2.54762 90) (size 2.09804 1.59766) (layers Top F.Paste F.Mask)
      (net 70 GNDPWR))
    (pad D+ smd rect (at 0 -2.67462 90) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 72 "Net-(R10-Pad1)"))
    (pad D- smd rect (at -0.6477 -2.67462 90) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 73 "Net-(R9-Pad1)"))
    (pad GND smd rect (at 1.29794 -2.67462 90) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad ID smd rect (at 0.6477 -2.67462 90) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 16 "Net-(X1-PadID)"))
    (pad VBUS smd rect (at -1.29794 -2.67462 90) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 21 "Net-(C4-Pad1)"))
  )
  (module PocketBeagle.pretty:MINI_PUSHBUTTON (layer Top) (tedit 5A71F5D0)
    (at 154.7368 98.49866 90)
    (attr smd)
    (fp_text reference SW1 (at 0.0254 -1.97866 90) (layer F.SilkS))
    (fp_text value BTN (at 0.80772 2.36474 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.99898 -0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 60 GPIO_BTN))
    (pad 2 smd rect (at 1.99898 -0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 60 GPIO_BTN))
    (pad 3 smd rect (at -1.99898 0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.99898 0.7493 90) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module "PocketBeagle.pretty:SON-6(TI)-DRY" (layer Top) (tedit 5A71F810)
    (at 137.287 112.014)
    (attr smd)
    (fp_text reference U3 (at 0.0889 -1.2192) (layer F.SilkS))
    (fp_text value TPD4S012DRY (at 2.16662 1.34112) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.49784 0.37846) (size 0.29972 0.51816) (layers Top F.Paste F.Mask)
      (net 66 USB1_D+))
    (pad 2 smd rect (at 0 0.37338) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 67 USB1_D-))
    (pad 3 smd rect (at 0.49784 0.37338) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 86 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at 0.49784 -0.37338) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0 -0.37338) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 15 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -0.49784 -0.37338) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 68 USB1_VBUS))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Top) (tedit 5A7540DB)
    (at 137.40892 97.05594 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 1.22936 1.1657 180) (layer F.SilkS))
    (fp_text value BC817 (at 0 2.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 7 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 8 "Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Top) (tedit 5A7540E0)
    (at 154.83302 111.74774 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.23234 1.14838 180) (layer F.SilkS))
    (fp_text value BC817 (at 0 2.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Top) (tedit 5A7540D7)
    (at 158.37408 111.76 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.27508 1.2192 180) (layer F.SilkS))
    (fp_text value BC817 (at 0 2.5 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.031 0.038 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 3 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers Top F.Paste F.Mask)
      (net 4 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "PocketBeagle.pretty:TH-2X18-(35MIL-DIA)-W_O-SILK" (layer Top) (tedit 59924F19)
    (at 148.5011 92.3036)
    (attr virtual)
    (fp_text reference P2 (at -18.6055 -3.15468 180) (layer F.SilkS))
    (fp_text value ~ (at 0 0) (layer F.SilkS))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(P2-Pad36)"))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(P2-Pad35)"))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(P2-Pad34)"))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 60 GPIO_BTN))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(P2-Pad32)"))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 SPI_nCS))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(P2-Pad30)"))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 SPI_CLK))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(P2-Pad28)"))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 SPI_MISO))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 RESET#))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 SPI_MOSI))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(P2-Pad24)"))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3V3))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(P2-Pad22)"))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(P2-Pad20)"))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(P2-Pad19)"))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(P2-Pad18)"))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(P2-Pad17)"))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(P2-Pad16)"))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(P2-Pad14)"))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(P2-Pad13)"))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 87 PWR#))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(P2-Pad11)"))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(P2-Pad10)"))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(P2-Pad9)"))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(P2-Pad8)"))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(P2-Pad7)"))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(P2-Pad6)"))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(P2-Pad5)"))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(P2-Pad4)"))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(P2-Pad2)"))
    (pad 1 thru_hole rect (at -21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 PWM_RED))
  )
  (gr_text USR (at 154.7749 95.2627) (layer F.SilkS))
  (gr_text RST (at 163.4871 95.2881) (layer F.SilkS))
  (gr_text PWR (at 159.0167 95.2627) (layer F.SilkS))
  (gr_text "m_w\nka6sox" (at 172.7581 99.5553 90) (layer B.SilkS))
  (gr_text "BaconBits\nRev. 1\n02-14-2018" (at 146.9771 104.6353 90) (layer B.SilkS))
  (gr_text e-ale.org (at 148.7551 88.5063) (layer F.SilkS))
  (gr_text "BaconBits Rev. 1" (at 149.11832 121.15546) (layer F.SilkS))
  (gr_text 35 (at 171.06138 119.13362) (layer F.SilkS))
  (gr_text 2 (at 125.20168 115.9891) (layer F.SilkS))
  (gr_text 1 (at 125.14072 118.5926) (layer F.SilkS))
  (gr_text 1 (at 125.24232 93.25864) (layer F.SilkS))
  (gr_line (start 131.0011 122.5036) (end 166.0011 122.5036) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.0011 87.5036) (end 131.0011 87.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.0011 97.5036) (end 131.0011 87.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.0011 97.5036) (end 121.0011 112.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.0011 112.5036) (end 121.0011 112.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.0011 112.5036) (end 166.0011 122.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.0011 112.5036) (end 176.0011 97.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.0011 97.5036) (end 176.0011 97.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text 2 (at 125.30328 90.65514) (layer F.SilkS))
  (gr_text 36 (at 171.0436 91.059) (layer F.SilkS))
  (gr_text 35 (at 171.1198 93.5736) (layer F.SilkS))
  (gr_text 36 (at 171.1452 116.4336) (layer F.SilkS))
  (zone (net 10) (net_name +3V3) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.9111 120.2563) (xy 123.7361 114.5413) (xy 131.4831 114.5413) (xy 131.4831 110.0963) (xy 123.7361 110.0963)
        (xy 123.7361 100.5713) (xy 131.6101 100.5713) (xy 131.6101 96.1263) (xy 123.7361 96.1263) (xy 126.9111 89.2683)
        (xy 170.0911 89.2683) (xy 173.2661 96.1263) (xy 173.2661 105.6513) (xy 170.9801 105.6513) (xy 170.9801 108.4453)
        (xy 173.2661 108.4453) (xy 173.2661 112.2553) (xy 170.9801 112.2553) (xy 170.9801 115.1763) (xy 173.2661 115.1763)
        (xy 170.0911 120.2563)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.9111 120.2563) (xy 123.7361 114.5413) (xy 131.3561 114.5413) (xy 131.3561 110.0963) (xy 123.7361 110.0963)
        (xy 123.7361 100.5713) (xy 131.4831 100.5713) (xy 131.4831 96.1263) (xy 123.7361 96.1263) (xy 126.9111 89.2683)
        (xy 170.0911 89.2683) (xy 173.2661 96.1263) (xy 173.2661 105.6513) (xy 170.9801 105.6513) (xy 170.9801 108.4453)
        (xy 173.2661 108.4453) (xy 173.2661 112.2553) (xy 170.9801 112.2553) (xy 170.9801 115.1763) (xy 173.2661 115.1763)
        (xy 170.0911 120.2563)
      )
    )
  )
  (zone (net 70) (net_name GNDPWR) (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.7111 85.9663) (xy 177.7111 124.0663) (xy 119.2911 124.0663) (xy 119.2911 85.9663)
      )
    )
  )
  (zone (net 70) (net_name GNDPWR) (layer Bottom) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.7111 85.9663) (xy 177.7111 124.0663) (xy 119.2911 124.0663) (xy 119.2911 85.9663)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.5387 110.6551) (xy 145.2753 110.6551) (xy 145.2753 112.3569) (xy 144.5387 112.3569)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.8887 110.6551) (xy 151.6253 110.6551) (xy 151.6253 112.3569) (xy 150.8887 112.3569)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.8633 106.2355) (xy 151.5999 106.2355) (xy 151.5999 107.9373) (xy 150.8633 107.9373)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.5133 106.2355) (xy 145.2499 106.2355) (xy 145.2499 107.9373) (xy 144.5133 107.9373)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.5387 102.0445) (xy 145.2753 102.0445) (xy 145.2753 103.7463) (xy 144.5387 103.7463)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.8887 102.0445) (xy 151.6253 102.0445) (xy 151.6253 103.7463) (xy 150.8887 103.7463)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.5387 97.6249) (xy 145.2753 97.6249) (xy 145.2753 99.3267) (xy 144.5387 99.3267)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.8887 97.6249) (xy 151.6253 97.6249) (xy 151.6253 99.3267) (xy 150.8887 99.3267)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.0373 107.9627) (xy 147.3327 107.9627) (xy 147.3327 110.6551) (xy 146.0373 110.6551)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.8313 107.9627) (xy 150.1267 107.9627) (xy 150.1267 110.6551) (xy 148.8313 110.6551)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.0373 99.3521) (xy 147.3327 99.3521) (xy 147.3327 102.0445) (xy 146.0373 102.0445)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.8313 99.3521) (xy 150.1267 99.3521) (xy 150.1267 102.0445) (xy 148.8313 102.0445)
      )
    )
  )
)
